How To Disable SNMPv2 Even In Default VRF And Keep SNMPv3 Enabled In ArubaOS-CX Devices?

**Labels: ArubaOS-CX 8400, ArubaOS-CX 8320**

**Q:**

Is it possible to keep SNMPv2 disabled and keep SNMPv3 enabled in Aruba-OSCX devices ?

**A:**

A new CLI command (snmp-server snmpv3-only) will be added in 10.07 software  
  
  
**6300(config)# snmp-server snmpv3-only**  
  
**This command will enable only snmpv3 and keep snmpv2 disabled.**  
  
6300# show ver  
-----------------------------------------------------------------------------  
ArubaOS-CX  
(c) Copyright 2017-2021 Hewlett Packard Enterprise Development LP  
-----------------------------------------------------------------------------  
**Version      : FL.10.07.0001CN**  
Build Date   : 2021-04-12 13:18:05 UTC  
Build ID     : ArubaOS-CX:FL.10.07.0001CN:904d421cb4f4:202104121220  
Build SHA    : 904d421cb4f49b2860c737e14cc6f5f57d918823  
Active Image : primary

Tags: ArubaOS-CX 8400, ArubaOS-CX 8320, arubaos-cx 8400x 10.00.0003, #arubaos-cx, #6300, #aos-cx, #snmpv2, #snmpv3, #vrf