Solarwinds Network Traffic Analyzer is using port UDP 2055, configure Sflow or NetFlow in router ?

**Labels: HPE Comware Switch**

**Q:**

Solarwinds Network Traffic Analyzer is using port UDP 2055, should we use Sflow or NetFlow in router

**A:**

**UDP port 2055 is one of the common netflow ports, so in router you should configure Netflow.**

Configuring Sflow in router would not help. Sflow uses default UDP port 6343.

**Neflow** is also known as**netstream**in HPE Comware devices. Hence in HPE Comware router configure netstream.

Tags: HPE Comware Switch, 10.02.0010, netstream, netflow, netflow collector, sflow, solarwinds